# IBM(c) 2007 EPL license http://www.eclipse.org/legal/epl-v10.html
#
# Raw commands to set BMCs to defaults
#   dx320
#     0x2e 0x10 0x4d 0x4f 0x00 0xff
#
#   dx340 
#     0x30 0x13 0xff 0x00 0x00 0x00
#
#   dx360/x3450
#     0x30 0x02 0x43 0x4c 0x52 0xaa
#     0x08 0x00 0x49 0x4e 0x54 0x45 0x4c
#     0x08 0x04
#
allowcred.awk &
CREDPID=$!
sleep 2
modprobe ipmi_si
modprobe ipmi_devintf
while [ -z "$BMCIP" ]; do
    while ! getipmi
    do
        echo "Retrying retrieval of IPMI settings from server"
    done
    TIMEOUT=15
    BMCIP=`grep bmcip /tmp/ipmi.data |awk -F\> '{print $2}'|awk -F\< '{print $1}'`
    BMCGW=`grep gateway /tmp/ipmi.data |awk -F\> '{print $2}'|awk -F\< '{print $1}'`
    BMCNM=`grep netmask /tmp/ipmi.data |awk -F\> '{print $2}'|awk -F\< '{print $1}'`
    BMCUS=`grep username /tmp/ipmi.data |awk -F\> '{print $2}'|awk -F\< '{print $1}'`
    BMCPW=`grep password /tmp/ipmi.data |awk -F\> '{print $2}'|awk -F\< '{print $1}'`
    if [ -z "$BMCIP" ]; then
        echo "FAILED TO RETRIEVE SETTINGS, RETRYING in 15 seconds"
        sleep 15
    fi
done
kill $CREDPID
NUMBMCS=`grep bmcip /tmp/ipmi.data |awk -F\> '{print $2}'|awk -F\< '{print $1}'|wc -l`
IPMIVER=`ipmitool mc info|grep ^IPMI|awk  '{print $4}'`
IPMIMFG=`ipmitool mc info|grep "^Manufacturer ID"|awk  '{print $4}'`
if [ "$IPMIMFG" == 2 ]; then #IBM
    XPROD=`ipmitool mc info|grep "^Product ID"|awk '{print $4}'`
    if [ "$XPROD" == "220" ]; then
        LOCKEDUSERS=1
        BMCPORT=`grep bmcport /tmp/ipmi.data |awk -F\> '{print $2}'|awk -F\< '{print $1}'`
        if [ ! -z "$BMCPORT" ]; then
	    let idev=NUMBMCS-1
	    for p in $BMCPORT; do
            	ipmitool -d $idev raw 0xc 1 1 0xc0 $p > /dev/null
            	ipmitool -d $idev raw 0x04 0x12 0x09 0x01 0x18 0x${p}1 0x00 > /dev/null
	    	let idev=idev-1
	    done
        fi
    else
        IBMFAM=`ipmitool raw 0x3a 0x50 |head -n 1| awk '{print $1 $2 $3 $4}'`
        if [ "$IBMFAM" == "59554f4f" ]; then
            BMCPORT=`grep bmcport /tmp/ipmi.data |awk -F\> '{print $2}'|awk -F\< '{print $1}'`
            if [ ! -z "$BMCPORT" ]; then
	    	let idev=NUMBMCS-1
		    for p in $BMCPORT; do
	            	ipmitool -d $idev raw 0xc 1 1 0xc0 $BMCPORT > /dev/null
		    	let idev=idev-1
		    done
            fi
        fi
    fi
elif [ "$IPMIMFG" == 20301 ] ; then
    XPROD=`ipmitool mc info|grep "^Product ID"|awk '{print $4}'`
    if [ "$XPROD" == "220" ]; then
        LOCKEDUSERS=1
        BMCPORT=`grep bmcport /tmp/ipmi.data |awk -F\> '{print $2}'|awk -F\< '{print $1}'`
        if [ ! -z "$BMCPORT" ]; then
	    	let idev=NUMBMCS-1
		    for p in $BMCPORT; do
	            	ipmitool -d $idev raw 0xc 1 1 0xc0 $BMCPORT > /dev/null
		    	let idev=idev-1
		    done
        fi
    fi
fi
echo -n "Auto detecting LAN channel..."

for LANCHAN in 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16; do 
   if ipmitool channel info $LANCHAN 2> /dev/null | grep 802.3 > /dev/null 2>&1 && ipmitool raw 0xc 2 $LANCHAN 5 0 0 > /dev/null 2>&1; 
     then break; 
   fi; 
   echo -n "."
done
echo "Detected LAN channel $LANCHAN"
        
let idev=NUMBMCS
while [ $idev -gt 0 ]; do
	let idev=idev-1
	TRIES=0
	while ! ipmitool -d $idev lan set $LANCHAN ipsrc static; do
	    sleep 1
	    let TRIES=TRIES+1
	    if [ $TRIES -gt $TIMEOUT ]; then break; fi
	done
done
let idev=NUMBMCS-1
for b in $BMCIP; do
	TRIES=0
	while ! ipmitool -d $idev lan set $LANCHAN ipaddr $b; do
	    sleep 1
	    let TRIES=TRIES+1
	    if [ $TRIES -gt $TIMEOUT ]; then break; fi
	done
	let idev=idev-1
done
let idev=NUMBMCS-1
for m in $BMCNM; do
	TRIES=0
	while ! ipmitool -d $idev lan set $LANCHAN netmask $m; do
	    sleep 1
	    let TRIES=TRIES+1
	    if [ $TRIES -gt $TIMEOUT ]; then break; fi
	done
	let idev=idev-1
done
TRIES=0
if [ ! -z "$BMCGW" ]; then
    let idev=NUMBMCS-1
    for g in $BMCGW; do
    	TRIES=0
	    while ! ipmitool -d $idev lan set $LANCHAN defgw ipaddr $g; do
	        sleep 1
	        let TRIES=TRIES+1
	        if [ $TRIES -gt $TIMEOUT ]; then break; fi
	    done
            let idev=idev-1
    done
    TRIES=0
fi
let idev=NUMBMCS-1
for bmcu in $BMCUS; do
DISABLEUSERS="1 2 3 4"
if [ ! -z "$LOCKEDUSERS" ]; then
    USERSLOT=`ipmitool -d $idev user list $LANCHAN |grep -v ^ID|awk '{print $1 " " $2}'|grep " $BMCUS"|awk '{print $1}'`
    if [ -z "$USERSLOT" ]; then
        USERSLOT=4
    fi
else
    USERSLOT=2
fi
CURRENTUSER=`ipmitool -d $idev user list $LANCHAN|grep ^$USERSLOT|awk '{print $2}'`
DISABLEUSERS=`echo 1 2 3 4|sed -e s/$USERSLOT//`
for user in $DISABLEUSERS; do
    while ! ipmitool -d $idev user disable $user; do
        sleep 1
        let TRIES=TRIES+1
        if [ $TRIES -gt $TIMEOUT ]; then break; fi
    done
    TRIES=0
done
TRIES=0
while ! ipmitool -d $idev user enable $USERSLOT; do
    sleep 1
    let TRIES=TRIES+1
    if [ $TRIES -gt $TIMEOUT ]; then break; fi
done
TRIES=0
# Last param in ipmitool user priv is the channel to set it on.
# Penguin boxes are all channel 2
CURRPRIV=`ipmitool -d $idev user list 1|grep ^$USERSLOT|awk '{print $6}'`
if [ "$CURRPRIV" != "ADMINISTRATOR" ]; then 
    while ! ipmitool -d $idev user priv $USERSLOT 4 $LANCHAN; do
        sleep 1
        let TRIES=TRIES+1
    if [ $TRIES -gt $TIMEOUT ]; then break; fi
    done
    TRIES=0
fi
if [ "$CURRENTUSER" != "$bmcu" ]; then
    while ! ipmitool -d $idev user set name $USERSLOT $bmcu; do
        sleep 1
        let TRIES=TRIES+1
        if [ $TRIES -gt $TIMEOUT ]; then break; fi
    done
fi
let idev=idev-1
done
let idev=NUMBMCS-1
for bmcp in $BMCPW; do
TRIES=0
while ! ipmitool -d $idev user set password $USERSLOT $bmcp; do
    sleep 1
    let TRIES=TRIES+1
    if [ $TRIES -gt $TIMEOUT ]; then break; fi
done
TRIES=0
echo "Set up following user table: "
ipmitool -d $idev user list $LANCHAN
let idev=idev-1
done

let idev=NUMBMCS
while [ $idev -gt 0 ]; do
let idev=idev-1


echo -n "Enabling Channel $LANCHAN: "
while ! ipmitool -d $idev raw 0x6 0x40 $LANCHAN 0x42 0x44 > /dev/null; do
    sleep 1
    let TRIES=TRIES+1
    if [ $TRIES -gt $TIMEOUT ]; then break; fi
done
TRIES=0
while ! ipmitool -d $idev raw 0x6 0x40 $LANCHAN 0x82 0x84 > /dev/null; do
    sleep 1
    let TRIES=TRIES+1
    if [ $TRIES -gt $TIMEOUT ]; then break; fi
done
if [ $TRIES -gt $TIMEOUT ]; then echo "ERROR"; else echo "OK"; fi
TRIES=0

echo -n "Enabling ARP responses: "
while ! ipmitool -d $idev lan set $LANCHAN arp respond on > /dev/null; do
    sleep 1
    let TRIES=TRIES+1
    echo -n .
    if [ $TRIES -gt $TIMEOUT ]; then break; fi
done
if [ $TRIES -gt $TIMEOUT ]; then echo "ERROR"; else echo "OK"; fi
TRIES=0

echo -n "Enabling IPMI v 1.5 MD5 LAN access:"
while ! ipmitool -d $idev lan set $LANCHAN auth admin md5 > /dev/null; do
    sleep 1
    let TRIES=TRIES+1
    if [ $TRIES -gt $TIMEOUT ]; then break; fi
done
if [ $TRIES -gt $TIMEOUT ]; then echo "ERROR"; else echo "OK"; fi
TRIES=0
if [ ! "$IPMIVER" == "1.5"  ]; then 
    echo -n "Enabling IPMI v 2.0 LAN access:"
    SUPPORTEDSUITES=`ipmitool -d $idev lan print $LANCHAN|grep Suites|awk -F: '{print $2}'|sed -e 's/ 0//'`
    PRIVS="X"
    for priv in 1 2 3 4 5 6 7 8 9 10 11 12 13 14; do
        if echo $SUPPORTEDSUITES|grep $priv > /dev/null; then
            PRIVS="$PRIVS"a
        else
            PRIVS="$PRIVS"X
        fi
    done
    while ! ipmitool -d $idev lan set $LANCHAN cipher_privs $PRIVS > /dev/null; do
        sleep 1
        let TRIES=TRIES+1
    if [ $TRIES -gt $TIMEOUT ]; then break; fi
    done
    if [ $TRIES -gt $TIMEOUT ]; then echo "ERROR"; else echo "OK"; fi
    TRIES=0

    echo -n "Enabling SOL for channel $LANCHAN:"
    while ! ipmitool -d $idev raw 0xc 0x21 $LANCHAN 0x1 0x1 > /dev/null; do
        sleep 1
        let TRIES=TRIES+1
        if [ $TRIES -gt $TIMEOUT ]; then break; fi
    done
    if [ $TRIES -gt $TIMEOUT ]; then echo "ERROR"; else echo "OK"; fi
    TRIES=0
    
    echo -n "Enabling SOL for $BMCUS:"
    while ! ipmitool -d $idev raw 6 0x4c $LANCHAN $USERSLOT 2 0 0 0 > /dev/null; do
        sleep 1
        let TRIES=TRIES+1
        if [ $TRIES -gt $TIMEOUT ]; then break; fi
    done
    if [ $TRIES -gt $TIMEOUT ]; then echo "ERROR"; else echo "OK"; fi
    echo -n "Putting SOL on channel $LANCHAN:"
    while ! OUTPUT=`ipmitool -d $idev raw 0xc 0x21 $LANCHAN 7 $LANCHAN 2>&1 > /dev/null`; do
	if echo $OUTPUT|grep "Unknown (0x80)" > /dev/null; then
		echo "Not Needed"
		break
        fi
        sleep 1
        let TRIES=TRIES+1
        if [ $TRIES -gt $TIMEOUT ]; then break; fi
    done
    if [ $TRIES -gt $TIMEOUT ]; then echo "ERROR"; else echo "OK"; fi
fi

#frume.awk

echo "Lighting Identify Light"
while :
    do ipmitool -d $idev raw 0 4 10 > /dev/null
    sleep 7
done &
done

