start:rvitals_h
description:get rvitals's usage
Attribute: $$CN-The operation object of rvitals command
cmd:rvitals -h 
check:rc==0
check:output=~Usage:
check:output=~rvitals
end

start:rvitals_v
description:get rvitals's version
Attribute: $$CN-The operation object of rvitals command
cmd:rvitals -v
check:rc==0
check:output=~Version
end

start:rvitals_temp
description:Retrieves temperatures
Attribute: $$CN-The operation object of rvitals command
cmd:/opt/xcat/share/xcat/tools/autotest/testcase/rvitals/openbmctest.sh rvitals $$CN temp
check:rc==0
end

start:rvitals_disktemp
description:Retrieves disk temperatures
Attribute: $$CN-The operation object of rvitals command
arch:ppc64le
hcp:ipmi
cmd:rvitals $$CN disktemp
check:rc==0
check:output=~Ambient Temp
end

start:rvitals_cputemp
description:Retrieves cpu  temperatures
Attribute: $$CN-The operation object of rvitals command
arch:ppc64le
hcp:ipmi
cmd:rvitals $$CN cputemp
check:rc==0
check:output=~Ambient Temp
end

start:rvitals_voltage
description:Retrieves power supply and VRM voltage readings
Attribute: $$CN-The operation object of rvitals command
cmd:/opt/xcat/share/xcat/tools/autotest/testcase/rvitals/openbmctest.sh rvitals $$CN voltage
check:rc==0
end

start:rvitals_power
description:Retrieves power status
Attribute: $$CN-The operation object of rvitals command
cmd:/opt/xcat/share/xcat/tools/autotest/testcase/rvitals/openbmctest.sh rvitals $$CN power
check:rc==0
end

start:rvitals_state
description:Retrieves the system state.
Attribute: $$CN-The operation object of rvitals command
cmd:rvitals $$CN state
check:rc==0
check:output=~System State:
end

start:rvitals_lcds
description:Retrieves LCDs status
Attribute: $$CN-The operation object of rvitals command
hcp:hmc,ivm,fsp,ipmi
cmd:rvitals $$CN lcds
check:rc==0
check:output=~Current LCD
end

start:rvitals_all
description:Retrieves all status
Attribute: $$CN-The operation object of rvitals command
cmd:/opt/xcat/share/xcat/tools/autotest/testcase/rvitals/openbmctest.sh rvitals $$CN all
check:rc==0
end

start:rvitals_leds
description:Retrieves leds status
Attribute: $$CN-The operation object of rvitals command
cmd:rvitals $$CN  leds
check:rc==0
check:output=~LED
end

start:rvitals_fanspeed
description:Retrieves fan speeds.
Attribute: $$CN-The operation object of rvitals command
cmd:/opt/xcat/share/xcat/tools/autotest/testcase/rvitals/openbmctest.sh rvitals $$CN fanspeed
check:rc==0
end
start:rvitals_wattage
description:Retrieves wattage readings.
Attribute: $$CN-The operation object of rvitals command
cmd:/opt/xcat/share/xcat/tools/autotest/testcase/rvitals/openbmctest.sh rvitals $$CN wattage
check:rc==0
end
start:rvitals_altitude
description:Retrieves altitude readings.
Attribute: $$CN-The operation object of rvitals command
cmd:/opt/xcat/share/xcat/tools/autotest/testcase/rvitals/openbmctest.sh rvitals $$CN altitude
check:rc==0
end
start:rvitals_noderange_err
description:using not defined node
cmd:/opt/xcat/share/xcat/tools/autotest/testcase/rvitals/openbmctest.sh rvitals testnode 
check:rc!=0
end
start:rvitals_errorcommand
description:using wrong command
cmd:/opt/xcat/share/xcat/tools/autotest/testcase/rvitals/openbmctest.sh rvitals $$CN errorcommand
check:rc!=0
end
