start:node_post
description: node_post
cmd:restapitest -m POST -r /nodes/node1 -d '{"groups":"all","mgt":"dfm","netboot":"yaboot"}'
check:rc==201
end

start:node_post2
description: node_post2
cmd:restapitest -m POST -r /nodes/node1 -d '{"groups":"all","mgt":"dfm","netboot":"yaboot"}'
check:rc==403
cmdcheck:restapitest -o '{"errorcode":"1"}' -O ==
end


start:node_put
description: node_put
cmd:restapitest -m PUT -r /nodes/node1 -d '{"mgt":"hmc","netboot":"xnba"}'
check:rc==200
end



start:nodes_get
description: nodes_get
cmd:restapitest -m GET -r /nodes
check:rc==200
cmdcheck:restapitest -o '["node1"]' -O ==
end

start:node_get
description: node_get
cmd:restapitest -m GET -r /nodes/node1
check:rc==200
cmdcheck:restapitest -o '{"node1":{"netboot":"xnba"}}' -O ==
end

start:node_delete
description: node_delete
cmd:restapitest -m DELETE -r /nodes/node1
check:rc==200
end

start:nodes_get2
description: nodes_get2
cmd:restapitest -m GET -r /nodes
check:rc==200
cmdcheck:restapitest -o '["node1"]' -O !=
end

start:node_get2
description: node_get2
cmd:restapitest -m GET -r /nodes/node1
check:rc==403
cmdcheck:restapitest -o '{"errorcode":"1"}' -O ==
end

start:node_post3_for_get_test
description: node_post3_for_get_test
cmd:restapitest -m POST -r /nodes/node1 -d '{"groups":"all","mgt":"dfm","netboot":"yaboot"}'
check:rc==201
end

start:node_attr_get
description: node_get2
cmd:restapitest -m GET -r /nodes/node1/attrs/mgt,groups,netboot
check:rc==200
cmdcheck:restapitest -o '{"node1":{"netboot":"yaboot"}}' -O ==
end

start:node_makehosts
description: node_makehosts
cmd:restapitest -m POST -r /nodes/node1/host
check:rc==201
end

start:node_makedns
description: node_makehosts
cmd:restapitest -m POST -r /nodes/node1/dns
check:rc==201
end


start:node_delete_dns
description: node_delete_dns
cmd:restapitest -m DELETE -r /nodes/node1/dns
check:rc==200
end

start:node_put
description: node_put
cmd:restapitest -m PUT -r /nodes/node1 -d '{"mac":"00:1a:64:54:14:80"}'
check:rc==200
end

start:node_makedhcp
description: node_makedhcp
cmd:restapitest -m POST -r /nodes/node1/dhcp
check:rc==201
end

start:node_delete_dhcp
description: node_delete_dhcp
cmd:restapitest -m DELETE -r /nodes/node1/dhcp
check:rc==200
end

start:node_state
description: node_state
cmd:restapitest -m GET -r /nodes/node1/nodestat
check:rc==200
cmdcheck:restapitest -o '{"node1":{"nodestat":"ANY"}}' -O ==
end


#start:node_post4_for_scan_test
#description: node_post4_for_scan_test
#cmd:restapitest -m POST -r /nodes/e108m6hmc02 -d '{"groups":"all,hmc","mgt":"hmc","hwtype":"hmc","mtm":"7042CR4","serial":"1050FBB","nodetype":"ppc"}'
#check:rc==201
#end

start:node_scan
description: node_scan
cmd:restapitest -m GET -r /nodes/__GETNODEATTR($$CN,hcp)__
check:rc==200
cmdcheck:restapitest -o '{"__GETNODEATTR($$CN,hcp)__":"ANY"}' -O ==
end


start:node_power_get
description: node_power_get
cmd:restapitest -m GET -r /nodes/$$CN/power
check:rc==200
cmdcheck:restapitest -o '{"$$CN":{"power":"ANY"}}' -O ==
end

start:node_power_put
description: node_power_reset
cmd:restapitest -m PUT -r /nodes/$$CN/power -d '{"action":"reset"}'
check:rc==200
end

#start:node_energy_put
#description: node_energy_put
#cmd:restapitest -m PUT -r /nodes/Vc68m5sn01/energy -d '{"cappingstatus":"on"}'
#check:rc==200
#end

#start:node_energy_get
#description: node_energy_get
#cmd:restapitest -m GET -r /nodes/Vc68m5sn01/energy 
#check:rc==200
#cmdcheck:restapitest -o '{"Vc68m5sn01":{"cappingmin":"on"}}' -O ==
#end

#start:node_energy_get_attr
#description: node_energy_get_attr
#cmd:restapitest -m GET -r /nodes/Vc68m5sn01/energy/cappingmaxmin,cappingstatus 
#check:rc==200
#cmdcheck:restapitest -o '{"Vc68m5sn01":{"cappingmin":"ANY"}}' -O ==
#end

#start:node_get_attr
#description: node_get_attr
#cmd:restapitest -m GET -r /nodes/Vc68m5sn01/sp/community
#check:rc==200
#cmdcheck:restapitest -o '{"Vc68m5sn01":{"SP SNMP Community":"public"}}' -O ==
#end

#start:node_put_attr
#description: node_put_attr
#cmd:restapitest -m PUT -r /nodes/Vc68m5sn01/sp/community -d '{"value":"mycommunity"}''
#check:rc==200
#end

#start:node_put_nextboot
#description: node_put_nextboot
#cmd:restapitest -m PUT -r /nodes/$$CN/nextboot -d '{"order":"net"}'
#check:rc==201
#end

#start:node_get_nextboot
#description: node_get_nextboot
#cmd:restapitest -m GET -r /nodes/Vc68m5sn01/nextboot 
#check:rc==200
#cmdcheck:restapitest -o '{"Vc68m5sn01":{"nextboot":"net"}}' -O ==
#end

start:node_put_bootstate
description: node_put_bootstate
cmd:restapitest -m PUT -r /nodes/Vc68m5sn01/bootstate -d '{"osimage":"rhels6.4-x86_64-install-compute"}'
check:rc==201
end

start:node_get_bootstate
description: node_get_bootstate
cmd:restapitest -m GET -r /nodes/$$CN/bootstate 
check:rc==200
cmdcheck:restapitest -o '{"$$CN":{"bootstat":"ANY"}}' -O ==
end

start:node_get_vitals
description: node_get_vitals
cmd:restapitest -m GET -r /nodes/Vc68m5sn01/vitals 
check:rc==200
cmdcheck:restapitest -o '{"Vc68m5sn01":{"SysBrd Fault":"0"}}' -O ==
end

start:node_get_vitals_attr
description: node_get_vitals_attr
cmd:restapitest -m GET -r /nodes/$$CN/vitals/all
check:rc==200
cmdcheck:restapitest -o '{"$$CN":{"System Temperature":"ANY"}}' -O ==
end

start:node_get_inventory
description: node_get_inventory
cmd:restapitest -m GET -r /nodes/Vc68m5sn01/inventory
check:rc==200
cmdcheck:restapitest -o '{"Vc68m5sn01":{"Power Supply 2 Board FRU Number":"94Y8105"}}' -O ==
end

start:node_get_inventory_attr
description: node_get_inventory_attr
cmd:restapitest -m GET -r /nodes/Vc68m5sn01/inventory/model
check:rc==200
cmdcheck:restapitest -o '{"Vc68m5sn01":{"System Description":"System x3650 M4"}}' -O ==
end

#start:node_get_eventlog
#description: node_get_eventlog
#cmd:restapitest -m GET -r /nodes/Vc68m5sn01/eventlog
#check:rc==200
#cmdcheck:restapitest -o '{"Vc68m5sn01":{"eventlog":"ANY"}}' -O ==
#end

start:node_post_nodecopy
description: node_post_nodecopy
cmd:restapitest -m POST -r /nodes/$$CN/nodecopy -d '{"src":["/etc/hosts","/etc/resolv.conf"],"target":"/tmp"}'
check:rc==201
end


