#!/bin/bash
CREDPID=$!
if [ -z "$XCATDEST" ]; then
	XCATDEST=$1
fi
if [ -z "$XCATDEST" ]; then
	for parm in `cat /proc/cmdline` ; do
		if echo $parm |grep xcatd= > /dev/null; then
			XCATDEST=`echo $parm |awk -F= '{print $2}'`
		fi
	done
fi
for LANCHAN in 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16; do 
   if ipmitool channel info $LANCHAN 2> /dev/null | grep 802.3 > /dev/null 2>&1 && ipmitool raw 0xc 2 $LANCHAN 5 0 0 > /dev/null 2>&1; 
     then break; 
   fi; 
done
BMCMAC=`ipmitool lan print $LANCHAN|grep ^MAC|awk '{print $4}'` #bmcconfig may opt to use DHCP, if so we need to feed up the mac address
#TODO: need a way to get the DUID the service processor may use, perhaps reserve that for 'ibmsetup' since spec doesn't touch ipv6?

echo "<xcatrequest>
<command>remoteimmsetup</command>
<bmcmac>$BMCMAC</bmcmac>
</xcatrequest>" > /tmp/bmcreq.xml
rm /tmp/remsetup.xml
while [ ! -f /tmp/remsetup.xml ] || grep error /tmp/remsetup.xml; do
	if [ -f /tmp/remsetup.xml ]; then
		timer=60
		while [ $timer -gt 0 ]; do
			sleep 1
			echo -en  "Retrying in $timer seconds  \r"
			timer=$(($timer-1));
		done
	fi
	echo -en "                                                         \r";
	
	if [ -f /etc/xcat/cert.pem -a -f /etc/xcat/certkey.pem ]; then #use client cert if available
		cat /tmp/bmcreq.xml | openssl s_client -key /etc/xcat/certkey.pem -cert /etc/xcat/cert.pem -connect $XCATDEST -quiet 2> /dev/null > /tmp/remsetup.xml
	else
		cat /tmp/bmcreq.xml | openssl s_client -connect $XCATDEST -quiet 2> /dev/null > /tmp/remsetup.xml
	fi
done
rm /tmp/bmcreq.xml
