start:rinv_mprom
description:this case is to test mprom option for rinv on x86_64 servers.
hcp:ipmi
arch:x86_64
cmd:rinv $$CN mprom 
check:rc==0
check:output=~BMC Firmware:\s*\w+.\w+
end

start:rinv_guid
description:this case is to test guid option for rinv on x86_64 servers.
hcp:ipmi
arch:x86_64
cmd:rinv $$CN guid 
check:rc==0
check:output=~UUID/GUID:\s*\w+-\w+-\w+-\w+-\w+
end

start:rinv_dimm
description:this case is to test dimm option for rinv on x86_64 servers.
hcp:ipmi
arch:x86_64
cmd:rinv $$CN dimm
check:rc==0
check:output=~DIMM 1 :\s*\w+
check:output=~DIMM 1 Manufacture Date:\s*\w+
check:output=~DIMM 1 Manufacture Location:\s*\d+
check:output=~DIMM 1 Model:\s*\w+-\w+
end
