start:rflash_check
description: Make sure the --check option works
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd:rflash $$CN --check
check:rc==0
check:output=~$$CN: BMC Firmware Product
check:output=~$$CN: HOST Firmware Product
end

start:rflash_invalid_activate
description: Provide an invalid option for activte, file does not end in .tar
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rflash $$CN -a /tmp/abc123.tz
check:rc==1
check:output=~Error: (\[.*?\]: )?Invalid firmware specified with -a
end

start:rflash_invalid_activate_and_delete
description: Cannot specify -a and --delete at the same time
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rflash $$CN -a 123 --delete 123
check:rc==1
check:output=~Error: (\[.*?\]: )?Multiple options are not supported
end

start:rflash_invalid_id
description: Passing an invalid ID to activate
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rflash $$CN -a 123
check:rc==1
check:output=~Error: (\[.*?\]: )?Invalid ID provided to activate
end

start:rflash_invalid_multiple_id_3
description: Code does not currently support multiple IDs to activate
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rflash $$CN -a 123 abc asdbas
check:rc==1
check:output=~Error: (\[.*?\]: )?More than one firmware specified is not supported
end

start:rflash_invalid_multiple_id_2
description: Code does not currently support multiple IDs to activate
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rflash $$CN -a asdbas 123
check:rc==1
check:output=~Error: (\[.*?\]: )?More than one firmware specified is not supported
end

start:rflash_invalid_node
description: Activate a valid ID hash but forget to put in a node range
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rflash -a 221d9020
check:rc==1
check:output=~Error: (\[.*?\]: )?Invalid nodes and/or groups in noderange: 221d9020
end

start:rflash_invalid_delete_2
description: Attempt to delete more than 1 ID from the FW
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rflash $$CN --delete 221d9020 221d9020
check:rc==1
check:output=~Error: (\[.*?\]: )?More than one firmware specified is not supported
end

start:rflash_delete_active_bmc
description: Attempt to delete the active BMC firmware
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rflash $$CN -l | grep \* | grep BMC | awk '{print $2}' | xargs -i{} rflash $$CN --delete {}
check:rc==1
check:output=~$$CN: (\[.*?\]: )?Error: Deleting currently active BMC firmware is not supported
end
