start:post_dns
description: post_dns
cmd:restapitest -m POST -r /services/dns
check:rc==201
end

start:post_dhcp
description: post_dhcp
cmd:restapitest -m POST -r /services/dns
check:rc==201
end

start:post_host
description: post_host
cmd:restapitest -m POST -r /services/host
check:rc==201
end

start:post_host
description: post_host
cmd:restapitest -m POST -r /services/host
check:rc==201
end

start:get_slpnodes
description: get_slpnodes
cmd:restapitest -m GET -r /services/slpnodes
check:rc==200
cmdcheck:restapitest -o '{"ngpcmm01":{"mpa":"ngpcmm01"}}' -O ==
end

start:get_slpnodes_withst
description: get_slpnodes_withst
cmd:restapitest -m GET -r /services/slpnodes/FSP
check:rc==200
cmdcheck:restapitest -o '{"Server--SNY014BG27A01K":{"mpa":"Server--SNY014BG27A01K"}}' -O ==
end



