#egan@us.ibm.com
#
cmdline

lang en_US
langsupport en_US
network --bootproto dhcp

#
# Where's the source?
# nfs --server hostname.of.server or IP --dir /path/to/RH/CD/image
#
#nfs --server #XCATVAR:INSTALL_NFS# --dir #XCATVAR:INSTALL_SRC_DIR#
#url --url http://#TABLE:noderes:$NODE:nfsserver#/install/#TABLE:nodetype:$NODE:os#/#TABLE:nodetype:$NODE:arch#

#INSTALL_SOURCES#

#device ethernet e100
keyboard "us"

#
# Clear the MBR
#
zerombr yes

#
# Wipe out the disk
#
clearpart --all --initlabel
#clearpart --linux

#
# Customize to fit your needs
#

#XCAT_PARTITION_START#
#No RAID
#/boot really significant for this sort of setup nowadays?
#part /boot --size 50 --fstype ext3
part swap --size 1024
part / --size 1 --grow --fstype ext3
#XCAT_PARTITION_END#

#RAID 0 /scr for performance
#part / --size 1024 --ondisk sda
#part swap --size 512 --ondisk sda
#part /var --size 1024 --ondisk sdb
#part swap --size 512 --ondisk sdb
#part raid.01 --size 1 --grow --ondisk sda
#part raid.02 --size 1 --grow --ondisk sdb
#raid /scr --level 0 --device md0 raid.01 raid.02

#Full RAID 1 Sample
#part raid.01 --size 50 --ondisk sda
#part raid.02 --size 50 --ondisk sdb
#raid /boot --level 1 --device md0 raid.01 raid.02
#
#part raid.11 --size 1024 --ondisk sda
#part raid.12 --size 1024 --ondisk sdb
#raid / --level 1 --device md1 raid.11 raid.12
#
#part raid.21 --size 1024 --ondisk sda
#part raid.22 --size 1024 --ondisk sdb
#raid /var --level 1 --device md2 raid.21 raid.22
#
#part raid.31 --size 1024 --ondisk sda
#part raid.32 --size 1024 --ondisk sdb
#raid swap --level 1 --device md3 raid.31 raid.32
#
#part raid.41 --size 1 --grow --ondisk sda
#part raid.42 --size 1 --grow --ondisk sdb
#raid /scr --level 1 --device md4 raid.41 raid.42

#
# bootloader config
# --append <args>
# --useLilo
# --md5pass <crypted MD5 password for GRUB>
#
bootloader

#
# install or upgrade
#
install

#
# text mode install (default is graphical)
#
text

#
# firewall
#
firewall --disabled

#
# mouse selection
#
#mouse genericps/2 --emulthree
mouse none

#
# Select a zone
# Add the --utc switch if your hardware clock is set to GMT
#
#timezone US/Hawaii
#timezone US/Pacific
#timezone US/Mountain
#timezone US/Central
#timezone US/Eastern
timezone --utc "#TABLE:site:key=timezone:value#"

#
# Don't do X
#
skipx


#
# To generate an encrypted root password use:
#
# perl -e 'print crypt("blah","Xa") . "\n";'p
# openssl passwd -apr1 -salt xxxxxxxx password
#
# where "blah" is your root password.
#
#rootpw --iscrypted XaLGAVe1C41x2
#rootpw XaLGAVe1C41x2 --iscrypted
rootpw --iscrypted #CRYPT:passwd:key=system,username=root:password#

#
# NIS setup: auth --enablenis --nisdomain sensenet
# --nisserver neptune --useshadow --enablemd5
#
# OR
auth --useshadow --enablemd5

#
# SE Linux
#
selinux --disabled

#
# Reboot after installation
#
reboot

#
#end of section
#
%packages --resolvedeps
#INCLUDE_DEFAULT_PKGLIST#
%pre
#INCLUDE:#ENV:XCATROOT#/share/xcat/install/scripts/pre.rh#
%post
#INCLUDE:#ENV:XCATROOT#/share/xcat/install/scripts/post.rh#
