# /etc/bootptab: database for QNX bootp server (/etc/bootpd)

# First, we define a global entry which specifies the stuff every host uses.
global:\
  :hd=/boot:\
  :ht=ethernet:\
  :sm=<your netmask here>:\
  :bf=|cd /boot; buildqnx -b 0x10000 build/<your build-file here> | mkQNXnbi:\
  :hn:

# node 2 uses the default build-file
node2:\
  :tc=global:\
  :ha=<your MAC here>:\
  :ip=<your IP address here>:

# node 3 uses its own build-file
node3:\
  :tc=global:\
  :ha=<your MAC here>:\
  :ip=<your IP address here>:\
  :bf=|cd /boot; buildqnx -b 0x10000 build/<your build-file here> | mkQNXnbi:

# node 4 uses a pre-built boot image
node3:\
  :tc=global:\
  :ha=<your MAC here>:\
  :ip=<your IP address here>:\
  :bf=images/<your image-file here>:
