start:rspconfig_record_firmware_level
description: Record the firmware level for the start of each testcase to display in the output
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rinv $$CN firm
check:rc==0
end

start:rspconfig_get_all_network
description: Check that we can get all the network related attributes from the BMC
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd:rspconfig $$CN ip netmask gateway hostname vlan
check:rc==0
check:output=~$$CN: BMC IP:
check:output=~$$CN: BMC Netmask:
check:output=~$$CN: BMC Gateway:
check:output=~$$CN: BMC Hostname:
check:output=~$$CN: BMC VLAN ID:
end

start:rspconfig_get_all_error
description: Check the parsing code for rspconfig (error cases)
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN ip,netmask,gateway,hostname,vlan
check:rc==1
check:output=~Error: (\[.*?\]: )?Unsupported command
end

start:rspconfig_get_set_error
description: Check the parsing code for rspconfig (error cases) - Cannot get/set in same line
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN ip netmask=255.0.0.0
check:rc==1
check:output=~Error: (\[.*?\]: )?Can not set and query OpenBMC information at the same time
end

start:rspconfig_get_and_set_hostname
description: Test setting and getting hostname on the BMC
os:Linux
hcp:openbmc
label:cn_bmc_ready,hctrl_openbmc
# Save the hostname to a file....
cmd:rspconfig $$CN hostname | tee /tmp/xcattest.rspconfig.hostname
check:rc==0
check:output=~$$CN: BMC Hostname:
# Set to witherspoon first
cmd:rspconfig $$CN hostname=witherspoon
check:rc==0
check:output=~$$CN: BMC Setting BMC Hostname...
# Check that it's set to witherspoon
cmd:rspconfig $$CN hostname
check:rc==0
check:output=~$$CN: BMC Hostname: witherspoon
# Set to <host>-UTset
cmd:rspconfig $$CN hostname=$$CN-UTset
check:rc==0
check:output=~$$CN: BMC Setting BMC Hostname...
# Check that it's set
cmd:rspconfig $$CN hostname
check:rc==0
check:output=~$$CN: BMC Hostname: $$CN-UTset
# Restore to saved version
cmd:grep BMC /tmp/xcattest.rspconfig.hostname  | cut -d' ' -f4 | xargs -i{} rspconfig $$CN hostname={}
check:rc==0
check:output=~$$CN: BMC Setting BMC Hostname...
cmd:rspconfig $$CN hostname
check:rc==0
check:output=~$$CN: BMC Hostname:
 AutoReboot
check:rc==0
end

start:rspconfig_admin_passwd_error
description: Check the error handling for changing of BMC password
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN admin_passwd=abc
check:rc==1
check:output=~$$CN: Error: Invalid parameter for option admin_passwd: abc
cmd: rspconfig $$CN admin_passwd=abc,xyz
check:rc==1
check:output=~Current BMC password is incorrect, cannot set the new password.
end

start:rspconfig_admin_passwd
description: Check the setting of BMC password to the same value
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN admin_passwd=0penBmc,0penBmc
check:rc==0
check:output=~$$CN: BMC Setting Password
end

start:rspconfig_autoreboot
description: Check the getting and setting of autoreboot attribute
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN autoreboot
check:rc==0
check:output=~$$CN: BMC AutoReboot
cmd: rspconfig $$CN autoreboot=0
check:rc==0
check:output=~$$CN: BMC Setting BMC AutoReboot
cmd: rspconfig $$CN autoreboot=1
check:rc==0
check:output=~$$CN: BMC Setting BMC AutoReboot
cmd: rspconfig $$CN autoreboot=
check:rc==1
check:output=~$$CN: Error: Invalid value '' for 'autoreboot', Valid values: 0,1
cmd: rspconfig $$CN autoreboot=2
check:rc==1
check:output=~$$CN: Error: Invalid value '2' for 'autoreboot', Valid values: 0,1
end

start:rspconfig_bootmode
description: Check the getting and setting of bootmode attribute
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN bootmode=safe
check:rc==0
check:output=~$$CN: BMC Setting BMC BootMode
cmd: rspconfig $$CN bootmode
check:rc==0
check:output=~$$CN: BMC BootMode: Safe
cmd: rspconfig $$CN bootmode=regular
check:rc==0
check:output=~$$CN: BMC Setting BMC BootMode
cmd: rspconfig $$CN bootmode=abc
check:rc==1
check:output=~$$CN: Error: Invalid value 'abc' for 'bootmode', Valid values: regular,safe,setup
end

start:rspconfig_dump
description: Check dump generation, download and removal
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
#Clear old dumps for this node
cmd: rm -f /var/log/xcat/dump/*$$CN*
#Generate new dump
cmd: rspconfig $$CN dump
check:rc==0
check:output=~Capturing BMC Diagnostic information, this will take some time
check:output=~$$CN: Dump requested. Target ID is
check:output=~Downloading dump
#Verify dump was downloaded to proper directory
cmd: ls -l /var/log/xcat/dump/*$$CN*
check:rc==0
#Remove last generated dump
cmd: rspconfig mid05tor12cn03 dump -l | tail -1 | cut -d ' ' -f2 | tr -d "[]" | xargs -i{} rspconfig $$CN dump -c {}
check:rc==0
check:output=clear
end

start:rspconfig_ntpservers
description: Check the getting and setting of ntpservers attribute
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN ntpservers
check:rc==0
check:output=~$$CN: BMC NTP Servers
cmd: rspconfig $$CN ntpservers=1.1.1.1
check:rc==0
check:output=~$$CN: BMC NTP Servers: 1.1.1.1
cmd: rspconfig $$CN ntpservers=
check:rc==0
check:output=~$$CN: BMC NTP Servers: None
end

start:rspconfig_powerrestorepolicy
description: Check the getting and setting of powerrestorepolicy attribute
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN powerrestorepolicy
check:rc==0
check:output=~$$CN: BMC PowerRestorePolicy
cmd: rspconfig $$CN powerrestorepolicy=always_on
check:rc==0
check:output=~$$CN: BMC Setting BMC PowerRestorePolicy
cmd: rspconfig $$CN powerrestorepolicy=always_off
check:rc==0
check:output=~$$CN: BMC Setting BMC PowerRestorePolicy
cmd: rspconfig $$CN powerrestorepolicy=restore
check:rc==0
check:output=~$$CN: BMC Setting BMC PowerRestorePolicy
cmd: rspconfig $$CN powerrestorepolicy
check:rc==0
check:output=~$$CN: BMC PowerRestorePolicy: Restore
cmd: rspconfig $$CN powerrestorepolicy=
check:rc==1
check:output=~$$CN: Error: Invalid value '' for 'powerrestorepolicy', Valid values: always_off,always_on,restore
cmd: rspconfig $$CN powerrestorepolicy=abc
check:rc==1
check:output=~$$CN: Error: Invalid value 'abc' for 'powerrestorepolicy', Valid values: always_off,always_on,restore
end

start:rspconfig_powersupplyredundancy
description: Check the getting and setting of powersupplyredundancy attribute
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN powersupplyredundancy=disabled
check:rc==1
check:output=~Error: 404 Not Found - Requested endpoint does not exist or may indicate function is not supported on this OpenBMC firmware.
cmd: rspconfig $$CN powersupplyredundancy
check:rc==0
check:output=~$$CN: BMC PowerSupplyRedundancy: Disabled
end

start:rspconfig_sshcfg
description: Check the copying of ssh keys to the BMC
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN sshcfg
check:rc==0
check:output=~$$CN: ssh keys copied to
end

start:rspconfig_timesyncmethod
description: Check the getting and setting of timesyncmethod attribute
hcp: openbmc
label:cn_bmc_ready,hctrl_openbmc
cmd: rspconfig $$CN timesyncmethod=manual
check:rc==0
check:output=~$$CN: BMC Setting BMC TimeSyncMethod
cmd: rspconfig $$CN timesyncmethod
check:rc==0
check:output=~$$CN: BMC TimeSyncMethod: Manual
cmd: rspconfig $$CN timesyncmethod=ntp
check:rc==0
check:output=~$$CN: BMC Setting BMC TimeSyncMethod
cmd: rspconfig $$CN timesyncmethod=abc
check:rc==1
check:output=~$$CN: Error: Invalid value 'abc' for 'timesyncmethod', Valid values: manual,ntp
end
